**Keyguard Data Form**

|  |
| --- |
|  |

**Identifier**:

Highlighted items must be provided or a screenshot, taken on the actual tablet, must be provided. Note a screenshot is always helpful even if the highlighted items are provided. It's also a good idea to include a picture of the app running on the tablet inside the case.

|  |  |  |
| --- | --- | --- |
| **Section & Option** | **Possible Values** | **My Value** |
| **Type of Tablet** | | |
| type of tablet: | **3D-Printed**, Laser-Cut |  |
| **Tablet** | | |
| type of tablet: | (see list below table) |  |
| orientation: | portrait, **landscape** |  |
| expose home button? | **yes**, no |  |
| expose camera? | **yes**, no |  |
| swap camera and home button? | yes, **no** |  |
| **Tablet Case** | | |
| have a case? | **yes**, no |  |
| height of opening in case: | 100 – 500 mm |  |
| width of opening in case: | 100 – 500 mm |  |
| case opening corner radius: | 0 – 30 mm |  |
| **App Layout & Bar Info** | | |
| status bar height: | 0 – 10 mm |  |
| expose status bar: | yes, **no** |  |
| upper message bar height: | 0 – 40 mm |  |
| expose upper message bar: | yes, **no** |  |
| upper command bar height: | 0 – 40 mm |  |
| expose upper command bar: | yes, **no** |  |
| lower message bar height: | 0 – 40 mm |  |
| expose lower message bar: | yes, **no** |  |
| lower message bar height: | 0 – 40 mm |  |
| expose lower message bar: | yes, **no** |  |
| lower command bar height: | 0 – 40 mm |  |
| expose lower command bar: | yes, **no** |  |
| bar edge slope: | 30 – 90 degrees |  |
| **Grid Layout** | | |
| number of columns: | 1 – 20 |  |
| number of rows: | 1 – 20 |  |
| horizontal rail width: | 3 – 25 mm |  |
| vertical rail width: | 3 – 25 mm |  |
| preferred rail height: | 2 – 15 mm |  |
| rail slope: | 30 – 90 degrees |  |
| shape of opening: | **rectangle**,  circle,  rounded rectangle |  |
| rounded rectangle corner radius: | 1 – 20 mm |  |
| cover these cells: | (start counting in lower left corner) |  |
| merge cells horizontally starting at: | (start counting in lower left corner) |  |
| merge cells vertically starting at: | (start counting in lower left corner) |  |
| add a ridge around these cells: | (start counting in lower left corner) |  |
| height of ridge: | 1 – 10 mm |  |
| thickness of ridge: | 1 – 10 mm |  |
| top padding: | -50 – 50 mm |  |
| bottom padding: | -50 – 50 mm |  |
| left padding: | -50 – 50 mm |  |
| right padding: | -50 – 50 mm |  |
| **Mounting Method** | | |
| mounting method: | **No Mount**, Suction Cups, Velcro,  Screw-on Straps, Clip-on Straps,  Slide-in Tabs - for cases, Raised Tabs - for cases, [Keyguard Frame] |  |
| **Velcro Info** | | |
| velcro size: | **10mm -3/8 in- Dots**, 16mm -5/8 in- Dots, 20mm -3/4 in- Dots, 3/8 in Squares, 5/8 in Squares, 3/4 in Squares |  |
| **Clip-on Straps Info** | | |
| clip locations: | **horizontal**, vertical, both |  |
| horizontal clip width: | 15 – 30 mm |  |
| vertical clip width: | 15 – 30 mm |  |
| distance between horizontal clip-on straps: | 20 – 120 mm |  |
| distance between vertical clip-on straps: | 20 – 120 mm |  |
| case width: | 200 – 400 mm |  |
| case height: | 200 – 400 mm |  |
| case thickness: | 5 – 40 mm |  |
| clip bottom length: | 15 – 45 mm |  |
| case to screen depth: | 1 – 10 mm |  |
| unequal left side of case: | 0 – 50 mm |  |
| unequal bottom side of case: | 0 – 50 mm |  |
| **Slide-in Tabs Info** | | |
| slide in tab locations: | **horizontal**, vertical, both |  |
| preferred slide in tab thickness: | 1 – 5 mm |  |
| horizontal slide in tab length: | 1 – 10 mm |  |
| vertical slide in tab length: | 1 – 10 mm |  |
| horizontal slide in tab width: | 10 – 200 mm |  |
| vertical slide in tab width: | 10 – 200 mm |  |
| distance between horizontal slide in tabs: | -10 – 120 mm |  |
| distance between vertical slide in tabs: | -10 – 120 mm |  |
| **Raised Tabs Info** | | |
| raised tab height: | 2 – 30 mm |  |
| raised tab length: | 3 – 30 mm |  |
| raised tab width: | 10 – 30 mm |  |
| preferred raised tab thickness: | 2 – 5 mm |  |
| starting height: | 0 – 5 mm |  |
| ramp angle: | 0 – 60 degrees |  |
| distance between raised tabs: | 0 – 150 mm |  |
| **Keyguard Frame Info** | | |
| have a keyguard frame? | yes, **no** |  |
| keyguard frame thickness | 4 – 10 mm |  |
| add a shelf? | yes, **no** |  |
| shelf thickness | 1 – 5 mm |  |
| shelf depth | 0 – 6 mm |  |
| **Free-form and Hybrid Keyguard** | | |
| free form keyguard thickness: | 3 – 10 mm |  |

Supported Tablets/Systems:

iPad

iPad2

iPad 3rd generation

iPad 4th generation

iPad 5th generation

iPad 6th generation

iPad 7th generation

iPad 8th generation

iPad 9th generation

iPad Pro 9.7-inch

iPad Pro 10.5-inch

iPad Pro 11-inch 1st Generation

iPad Pro 11-inch 2nd Generation

iPad Pro 11-inch 3rd Generation

iPad Pro 12.9-inch 1st Generation

iPad Pro 12.9-inch 2nd Generation

iPad Pro 12.9-inch 3rd Generation

iPad Pro 12.9-inch 4th Generation

iPad Pro 12.9-inch 5th Generation

iPad mini

iPad mini 2

iPad mini 3

iPad mini 4

iPad mini 5

iPad mini 6

iPad Air

iPad Air 2

iPad Air 3

iPad Air 4

Dynavox I-12+

Dynavox Indi

NovaChat 5

NovaChat 8

NovaChat 10

NovaChat 12

Chat Fusion 10

Surface 2

Surface 3

Surface Pro 3

Surface Pro 4

Surface Pro 5

Surface Pro 6

Surface Pro 7

Surface Pro X

Surface Go

Accent 800

Accent 1000

Accent 1400 AC14-20

Accent 1400 AC14-30

GridPad 12

GridPad 13

Amazon Fire HD 7

Amazon Fire HD 8

Amazon Fire HD 8 Plus

Amazon Fire HD 10

*Special Instructions:*

|  |
| --- |
|  |

|  |
| --- |
| **Tablet** |
| **Tablet Case** |
| **App Layout** |
| **Grid Layout** |

**3D Print Information**

Filament Type:

Outlines/Perimeters/Shells:

Number of Top and Bottom Solid Layers:

Layer Height (other than first layer):

Infill Percentage:

Printed with Supports?

Special Instructions: