**6th Finger and Toe Stylus**

**Design ID:**

(all measurements in millimeters)

|  |  |  |  |
| --- | --- | --- | --- |
| Option | Default Value | Possible Values | Notes |
| **Parts and Assembly** | | | |
| assembly type | dovetails | dovetails, all solid, solid rings |  |
| ring width | 10 | 4 to 15 |  |
| ring thickness | 2 | 1, 1.5, 2, 2.5, 3, 3.5 |  |
| stylus ring to stylus tip attachment angle | 0 | 0, 90 | 90 can only be used with conductive filament |
| stylus tip mount angle | 180 | 50 to 310 | this is the angle between the second ring and the stylus tip |
| dovetail joint tightness | 0 | -10 to 10 | affects only the male side of a dovetail joint |
| **Stylus Info** | | | |
| stylus width | 10 | 8 to 15 |  |
| conduction type | bolt and nut | bolt and nut, conductive filament |  |
| *---Conductive Stylus Info* | | | |
| stylus extender or stylus tip length | 20 | 10 to 200 |  |
| use 4mm nut to mount tip | no | yes, no | stylus width must be at least 10 |
| *---Bolted Stylus Info* | | | |
| bolt length | 25 | 20, 25, 30, 35, 40, 45, 50, 55, 60, 65, 70, 75, 80 |  |
| coupling nut length | 8 | 8, 15 |  |
| **Ring Info** | | | |
| finger or toe diameter | 20 | 5 to 30 |  |
| split ring | no | yes, no | does not apply to a stylus ring |
| stylus ring type | one finger ring | one finger ring, two finger rings | does not apply to a solid stylus |
| finger ring type | single finger ring | single finger ring, mount for second finger ring | does not apply to a solid stylus |
| **Solid Stylus Info** | | | |
| stylus ring diameter | 20 | 5 to 30 |  |
| number of finger toe rings | 1 | 1, 2 |  |
| finger/toe ring 1 diameter | 20 | 5 to 30 |  |
| finger/toe ring 2 diameter | 20 | 5 to 30 |  |
| **Mount Info** | | | |
| stylus tip diameter | 10 | 7 to 10 |  |
| holster opening height | 8 | 5 to 30 |  |
| holster opening diameter | 35 | 20 to 50 |  |
| shelf thickness | 25 | 10 to 60 |  |
| jaw length | 35 | 20 to 60 |  |